Poznamky z chapter 11

NAT-enabled router translates the internal IPv4 address of the device to a public address from the NAT pool.





